# Sensors Hookup Connector – 4 pins

Round IP66 connector, 4 pins.

1. +5V
2. +3.3V
3. Data
4. GND